\* 10 AMP

28 VDC

0.25 AMP

HIGH VOLTAGE

SL-BL

8 AMP

18 VDC

2.5 AMP

28 VDC

SL-BL

4 AMP

+5 VDC

LOGIC

SL-BL

FLIPPERS

DISPLAYS

LAMPS

SOLENOIDS

\* GAMES WITH MORE THAN THREE FLIPPERS USE 15A FUSE  
ABOVE FUSES LOCATED ON POWER SUPPLY

BELOW FUSES LOCATED ON FUSE CARD

4 AMP

19 VAC

SL-BL

20 AMP

6,3 VAC

4 AMP

19 VAC

SL-BL

GENERAL

ILLUMINATION

5V LOGIC SUPPLY

STD-624

Fonts used: Futura Md BT.

Fuse card STD-624 confirmed (size 111x96mm).

If you have any more fuse labels, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.