###### WARNING

**FOR SAFETY AND PROPER GAME OPERATION, GAME  
MUST BE PLUGGED INTO A PROPERLY GROUNDED  
OUTLET. 117 VAC 60 HZ.**

**THIS EQUIPMENT HAS NOT BEEN TESTED TO SHOW  
COMPLIANCE WITH NEW FCC RULES (47 CFR PART 15)  
DESIGNED TO LIMIT INTERFERENCE TO RADIO AND TV  
RECEPTION OPERATION OF THIS EQUIPMENT IN A  
RESIDENTIAL AREA IS LIKELY TO CAUSE UNACCEPT-  
ABLE INTERFERENCE TO RADIO COMMUNICATION  
REQUIRING THE OPERATOR TO TAKE WHATEVER  
STEPS ARE NECESSARY TO CORRECT THE INTER-  
FERENCE.**

###### STD-A707

Fonts used: Helvetica LT Std Cond Blk, Futura Std Medium,

Card size: 146x89mm

**Cards status:**

STD-A707 confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.