D–12247  
–566

16–8587–1012

AUX. PWR. FUSE LABEL

ROLLERGAMES

F3 2.5 ASB

F1 5 ASB

F2A  
 2.5 ASB

F2C 5 ASB

F4 7 ASB

F5 2 ASB

F6 2 ASB

F8 7 ASB

F7 4 ASB

D–12247  
–566  
(571)

16–8587–1012–1

AUX. PWR. FUSE LABEL

F3 2.5 ASB

F1 2.5 ASB

F2A  
 2.5 ASB

F2C 5 ASB

F4 2.5 ASB

F5 2 ASB

F6 2 ASB

F8 7 ASB

F7 4 ASB

Fonts used: Helvetica.

Card size: 82x114mm

Fuse card 16-8587-1012 confirmed.

Fuse card 16-8587-1012-1 confirmed. F1 and F4 adjusted.

If you have any more fuse labels, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.