###### 3 OUTS PER INNING

###### 1 INNING PER PLAY

FOR  
AMUSEMENT  
ONLY

UPPER DECK BASEBALL

###### 423-1

INNING  
VOID  
IF TILTED

###### 12 RUNS .................. 1 REPLAY

###### 18 RUNS .................. 1 REPLAY

###### 3 OUTS PER INNING

###### 2 INNINGS PER PLAY

FOR  
AMUSEMENT  
ONLY

UPPER DECK BASEBALL

###### 423-2

INNING  
VOID  
IF TILTED

###### 18 RUNS .................. 1 REPLAY

###### 24 RUNS .................. 1 REPLAY

###### 14 RUNS .................. 1 REPLAY

###### 26 RUNS .................. 1 REPLAY

###### 423-5

###### 22 RUNS .................. 1 REPLAY

###### 34 RUNS .................. 1 REPLAY

###### 423-6

###### 18 RUNS ......... 1 EXTRA INNING

###### 42 RUNS ......... 1 EXTRA INNING

###### 423-17

###### \_\_\_\_ RUNS ......... 1 EXTRA INNING

###### \_\_\_\_ RUNS ......... 1 EXTRA INNING

###### 423-18

TO REMOVE PLAYFIELD

**LOOSEN (2) WING NUTS, THEN TURN HOLDING BRACKET IN.**

423-13

INSTRUCTIONS

###### • INSERT COIN TO START GAME

###### 

###### • INSERT 2nd COIN FOR 2 PLAYERS

###### 423-21

INSTRUCTIONS

###### INSERT COIN TO START GAME

###### INSERT 2nd COIN FOR 2 PLAYERS

###### 423-22

###### INNING ADJUSTMENT

###### 1

###### 2

###### 3

###### 423-11

###### 3rd GRAND SLAM ....... 1 REPLAY

###### 423-23

###### 3rd Grand Slam ....... 1 Extra Inning

###### 423-24

###### 423-6

###### NORMAL

###### CONSERVATIVE

###### NORMAL- CONSERV. ADJUSTMENT

###### CREDIT

###### ADJUSTMENT

###### EXTRA INNING

###### 423-7

###### BLU-W GRAND SLAM

###### B-O HI-SCORE ADJ.

###### 423-12

###### GRAND SLAM ADJUSTMENT

###### 3 6 9

###### 423-8

###### 3 RD OUT RELAY

###### Z-27-1000

###### 423-10

###### 423-9

###### 1 2 3

###### GRAND SLAM SCORE ADJUSTMENT

###### HOME RUN RELAY M-30-1400

###### NO. 1 RELAY M-29-1100

###### NO. 2 RELAY M-29-1100

###### NO. 3 RELAY M-29-1100

###### Attach to the next strip at the dotted line.

###### NO. 4 RELAY M-29-1100

###### GRAND SLAM RELAY M-30-1400

###### 423-1

###### OUT RELAY M-29-1100

###### Attach to the next strip at the dotted line.

###### LOCK RELAY Z-28-1200

###### LOAD RELAY Z-28-1150

###### TILT RELAY Z-28-1150

###### COIN RELAY Z-28-1000

###### START RELAY Z-27-1000

###### SWING RELAY Z-28-1150

###### 423-2

###### BAT RELAY Z-28-1150

###### PITCH RELAY Z-28-1150

###### STRIKE RELAY M-30-1400

###### 423-3

###### BAT BUTTON RELAY M-29-1100

1 2

PLAY PLAYS

10c

COIN ADJ.

STD. 79

###### SLAM SWITCH CONTACTS NORMALLY CLOSED

STD. 400

**25**¢

**ADJ.**

5

4

3

2

STD. 446

NOTICE

THIS GAME OPERATES

ON **24 VOLTS**

###### STD. 8A

MOTOR-SERVICE JACK

ON OFF

**STD. 99**

BAT UNIT

END OF STROKE  
SWITCH OPENS  
CIRCUIT TO BAT  
RELAY.

STD. 428

HI-SCORE ADJUSTMENT

PLUG IN RED  
WIRE FOR SCORES  
11 TO 20

PLUG IN BLUE  
WIRE FOR SCORES  
21 TO 30

PLUG IN YELLOW  
WIRE FOR SCORES  
31 TO 40

PLUG IN GREEN  
WIRE FOR SCORES  
41 TO 50

EXAMPLE :

BLUE WIRE INTO 1 POSITION SCORES AT 21 OR  
BLUE WIRE INTO 0 POSITION SCORES AT 30.

400-6

POINT SCORE STORAGE  
ADJUSTMENT AREA

1

2

3

4

5

6

7

8

9

0

###### DECREASE INCREASE

###### BAT POWER

###### CONTROL

###### 370-12

UPPER DECK SOUND UNIT- 20A-9038

WE 1020

UA10

FUSE ¼ AMP

5A-8745

GM123

GM108

GM144-2

SIREN

CROWD

EXPLOSION

AMPLIFIER

16C-423-5

Fonts used: Alternate Gothic No.2, Helvetica Inserat LT Std, HelveticaNeue, Helvetica LT Std, Futura Md BT,   
Century, Futura Hv BT, Helvetica 55 Roman, News Gothic Demi

Card sizes: score cards 95x54mm, score inserts 95x24mm, instruction cards 95x54mm, insert strips 95x17mm

**Cards status:**

All card, inserts and labels confirmed.

If you have any other information about these cards, please send a readable picture or scan to me.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.