**FUSE**

**1 AMP SLO-BLO**

**STD-868**

**FUSE**

**1 AMP SLO-BLO**

**STD-868**

**FUSE**

**1 AMP SLO-BLO**

**STD-868**

**FUSE**

**2.5 AMP SLO-BLO**

**STD-882**

**FUSE**

**2.5 AMP SLO-BLO**

**STD-882**

**FUSE**

**2.5 AMP SLO-BLO**

**STD-882**

**FUSE**

**4.0 AMP SLO-BLO**

**STD-883**

**FUSE**

**4.0 AMP SLO-BLO**

**STD-883**

**FUSE**

**4.0 AMP SLO-BLO**

**STD-883**

**FUSE**

**4 AMP SLO-BLO**

**STD-914**

**FUSE**

**4 AMP SLO-BLO**

**STD-914**

**FUSE**

**4 AMP SLO-BLO**

**STD-914**

**FUSE**

**5 AMP SLO-BLO**

**STD-869**

**FUSE**

**5 AMP SLO-BLO**

**STD-869**

**FUSE**

**5 AMP SLO-BLO**

**STD-869**

**FUSE**

**0.25 AMP SLO-BLO**

**STD-924**

**FUSE**

**0.25 AMP SLO-BLO**

**STD-924**

**FUSE**

**0.25 AMP SLO-BLO**

**STD-924**

**2.5 A.S.B.**

**STD-943**

**2.5 A.S.B.**

**STD-943**

**2.5 A.S.B.**

**STD-943**

**8 AMP**

**STD-926**

**8 AMP**

**STD-926**

**8 AMP**

**STD-926**

**1/10 AMP**

**1/10 AMP**

**STD-923**

**1/10 AMP**

**1/10 AMP**

**STD-923**

**1/10 AMP**

**1/10 AMP**

**STD-923**

**0.1 AMP**

**0.1 AMP**

**STD-923’**

**0.1 AMP**

**0.1 AMP**

**STD-923’**

**0.1 AMP**

**0.1 AMP**

**STD-923’**

**7A SB**

**7A SB**

**STD-925**

**7A SB**

**7A SB**

**STD-925**

**7A SB**

**7A SB**

**STD-925**

LINE FUSE  
4 AMP FOR 220 V.  
8 AMP FOR 117 V.

**STD. 612**

LINE FUSE  
4 AMP FOR 220 V.  
8 AMP FOR 117 V.

**STD. 612**

LINE FUSE  
4 AMP FOR 220 V.  
8 AMP FOR 117 V.

**STD. 612**

**LINE FUSE  
4 AMP FOR 220 V.  
7½ AMP FOR 117 V.**

**STD. 581**

**LINE FUSE  
4 AMP FOR 220 V.  
7½ AMP FOR 117 V.**

**STD. 581**

**LINE FUSE  
4 AMP FOR 220 V.  
7½ AMP FOR 117 V.**

**STD. 581**

**BOTH SOUND  
FUSES:**

**4 amp** MDL

**STD-595**

**BOTH SOUND  
FUSES:**

**4 amp** MDL

**STD-595**

**BOTH SOUND  
FUSES:**

**4 amp** MDL

**STD-595**

**BOTH SOUND  
FUSES:**

**4 amp** MDL

**STD-595**

Fonts used: Helvetica LT Std Cond, Helvetica, Futura Medium, Futura Md BT, Times New Roman.

Fuse label STD-926 confirmed (44x11mm).

Fuse label STD-868 confirmed (44x11mm).

Fuse label STD-882 confirmed (44x11mm).

Fuse label STD-883 confirmed (44x11mm).

Fuse label STD-914 confirmed (44x11mm).

Fuse label STD-869 confirmed (44x11mm).

Fuse label STD-923 confirmed (44x25mm).

Fuse label STD-923’ is the same as STD-923, but has been adjusted to show 0.1A (44x25mm).

Fuse label STD-924 confirmed (44x12mm).

Fuse label STD-925 confirmed (44x25mm).

Fuse label STD-612 confirmed (50x19mm).

Fuse label STD-581 confirmed (50x19mm).

Fuse label STD-595 confirmed (37x19mm).

If you have any more fuse labels, please send me an image.

Enjoy and have fun,

Peter

[www.inkochnito.nl](http://www.inkochnito.nl)

If you like my work, please send me a donation via PayPal.